FLOOR DRAINS

SUGGESTED SPECIFICATIONS

Jay R. Smith Mfg. Co. has developed the following paragraphs to assist the design professional in specifying floor drains. Insert these paragraphs into project specification Section 22 40 00 - Plumbing Fixtures or other similarly titled section.

Notes are included to assist the design professional in editing the specifications to suit project requirements, and are not intended to be included in the final specification. These notes appear in blue text.

For assistance on the selection of the products in this section or for other questions, contact Jay R. Smith Mfg. Co. by calling 334-277-8520, by email at salesengineering@jrsmith.com, or visit our website at www.jrsmith.com.

PART 1 - GENERAL

Insert the following paragraphs under “Submittals”:

	A.	Review Submittals:
		1.	Product Data: Manufacturer’s standard data sheets describing components including materials, dimensions, relationship to adjacent construction, and attachments.

PART 2 - PRODUCTS

Insert the following under “Manufacturers”. Edit to indicate whether or not substitutions will be permitted for the products in this section.

	A.	Contract Documents are based on products by Jay R. Smith Mfg. Co.

	B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

Insert the following under “Components.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting specific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a basement floor drain.

	A.	Floor Drain:
1.	Model: No. 2220.

1.	Description: Cast Iron 8-1/2 inch diameter drain with light duty cast iron grate and cast iron  “safe-set” bucket.

**** OR ****

Include the following for a side outlet basement floor drain.

	A.	Floor Drain:
		1.	Model: No. 2225.
		2.	Description: Cast Iron, 8-1/2 inch diameter, side outlet drain with light duty cast iron grate and cast iron “safe-set” bucket.

**** OR ****

Include the following for a battery room floor drain.

	A.	Floor Drain:
		1.	Model: No. 9710, CF8 rough finish.
		2.	Description: Stainless steel body with loose set non-tilt medium duty stainless steel grate for use in floors where corrosive liquids will be drained or dumped.

**** OR ****

Include the following for a boiler room floor drain.

	A.	Floor Drain:
		1.	Model: No. 2495.
		2.	Description: Cast iron 8-1/2 inch diameter drain with heavy duty cast iron tractor grate and cast iron bucket.

**** OR ****

Include the following for a corridor or hallway floor drain.

	A.	Floor Drain:
		1.	Model: No. 2010 (-D-U).
		2.	Description: Cast iron drain with 7 inch adjustable nickel bronze strainer head. 

**** OR ****

Include the following for a side outlet corridor or hallway floor drain.

	A.	Floor Drain:
		1.	Model: No. 2015 (-D-U).
		2.	Description: Cast iron, side outlet, drain with 7 inch adjustable nickel bronze strainer head. 

**** OR ****

Include the following for a covered walkway floor drain.

	A.	Floor Drain:
		1.	Model: No. 2320 (-G-U).
		2.	Description: Galvanized cast iron 8-1/2 inch diameter drain with vandal proof medium duty galvanized cast iron tractor grate and cast iron adjustable top. 

**** OR ****

Include the following for a side outlet covered walkway floor drain.

	A.	Floor Drain:
		1.	Model: No. 2325 (-G-U).
		2.	Description: Galvanized cast iron, side outlet, 8-1/2 inch diameter drain with vandal proof medium duty galvanized cast iron tractor grate and cast iron adjustable top. 

**** OR ****

Include the following for a side wall elevator pit floor drain.

	A.	Floor Drain:
		1.	Model: No. 7000.
		2.	Description: Vertical inlet cast iron drain and secured cast iron grate with cast bronze backwater valve. 

**** OR ****

Include the following for a factory floor drain where normal waste is anticipated.

	A.	Floor Drain:
		1.	Model: No. 2450.
		2.	Description: Galvanized fabricated steel drain body with heavy duty cast iron tractor grate and stainless steel ported bucket. 

**** OR ****

Include the following for a side outlet factory floor drain where normal waste is anticipated.

	A.	Floor Drain:
		1.	Model: No. 2455.
		2.	Description: Galvanized fabricated steel, side outlet, drain body with heavy duty cast iron tractor grate and stainless steel ported bucket. 

**** OR ****

Include the following for a factory floor drain where fine sediment waste is anticipated.

	A.	Floor Drain:
		1.	Model: No. 2450.
		2.	Description: Cast iron drain with heavy duty tractor grate and sediment bucket with stainless steel mesh overflow ports. 

**** OR ****

Include the following for a floor drain where medium traffic and drainage are anticipated.

	A.	Floor Drain:
		1.	Model: No. 2340 (-B).
		2.	Description: Cast iron 12 inch diameter adjustable drain with cast iron sediment bucket and heavy duty cast iron tractor grate.

**** OR ****

Include the following for a side outlet floor drain where medium traffic and drainage are anticipated.

	A.	Floor Drain:
		1.	Model: No. 2345 (-B).
		2.	Description: Cast iron, side outlet, 12 inch diameter adjustable drain with cast iron sediment bucket and heavy duty cast iron tractor grate.

**** OR ****

Include the following for a floor drain where heavy traffic and light drainage are anticipated.

	A.	Floor Drain:
		1.	Model: No. 2120.
		2.	Description: Cast iron 8-1/2 inch diameter drain with heavy duty cast iron tractor grate.

**** OR ****

Include the following for a side outlet floor drain where heavy traffic and light drainage are anticipated.

	A.	Floor Drain:
		1.	Model: No. 2125.
		2.	Description: Cast iron, side outlet, 8-1/2 inch diameter drain with heavy duty cast iron tractor grate.

**** OR ****

Include the following for a floor drain where heavy traffic and drainage are anticipated.

	A.	Floor Drain:
		1.	Model: No. 2143.
		2.	Description: Cast iron 15 inch diameter drain with heavy duty cast iron tractor grate.

**** OR ****

Include the following for a floor drain where heavy traffic and heavy debris drainage are anticipated.

	A.	Floor Drain:
		1.	Model: No. 2253.
		2.	Description: Cast iron 15 inch diameter drain with slotted cast iron sediment bucket and heavy duty cast iron tractor grate.

**** OR ****

Include the following for a side outlet floor drain where heavy traffic and heavy debris drainage are anticipated.

	A.	Floor Drain:
		1.	Model: No. 2255.
		2.	Description: Cast iron, side outlet, 15 inch diameter drain with slotted cast iron sediment bucket and heavy duty cast iron tractor grate.

**** OR ****

Include the following for a flower box drain.

	A.	Floor Drain:
		1.	Model: No. 2670 (-G).
		2.	Description: Galvanized cast iron drain with cast bronze secured dome with stainless steel mesh screen and flashing collar.

**** OR ****

Include the following for a garage floor drain where light traffic is anticipated.

	A.	Floor Drain:
		1.	Model: No. 2233 (-G).
		2.	Description: Galvanized cast iron 12 inch diameter drain with slotted cast iron sediment bucket and heavy duty galvanized cast iron tractor grate.

**** OR ****

Include the following for a side outlet garage floor drain where light traffic is anticipated.

	A.	Floor Drain:
		1.	Model: No. 2238 (-G).
		2.	Description: Galvanized cast iron, side outlet, 12 inch diameter drain with slotted cast iron sediment bucket and heavy duty galvanized cast iron tractor grate.

**** OR ****

Include the following for a garage floor drain where heavy traffic is anticipated.

	A.	Floor Drain:
		1.	Model: No. 2250.
		2.	Description: Cast iron 16 inch diameter drain with slotted sediment bucket and heavy duty cast iron tractor grate.

**** OR ****

Include the following for a side outlet garage floor drain where heavy traffic is anticipated.

	A.	Floor Drain:
		1.	Model: No. 2255.
		2.	Description: Cast iron, side outlet, 16 inch diameter drain with slotted sediment bucket and heavy duty cast iron tractor grate.

**** OR ****

Include the following for a garbage can wash floor drain.

	A.	Floor Drain:
		1.	Model: No. 2690.
		2.	Description: Galvanized cast iron drain with slotted sediment bucket, flashing collar, cast iron grate and pipe sleeve. Bronze adjustable spray nozzle complete with 1/2 inch I.P.S. water connection assembly.

**** OR ****

Include the following for a market vegetable preparation room floor drain.

	A.	Floor Drain:
		1.	Model: No. 3041 (-19).
		2.	Description: Cast iron 8-1/2 inch diameter sanitary drain with acid resistant coated interior, aluminum sediment bucket, nickel bronze rim and nickle bronze hinged grate.

**** OR ****

Include the following for a market meat preparation room floor drain.

	A.	Floor Drain:
		1.	Model: No. 3020.
		2.	Description: Cast iron 8-1/2 inch diameter sanitary drain with acid resistant coated interior, aluminum dome bottom strainer, nickel bronze rim and nickle bronze secured grate.

**** OR ****

Include the following for a market refrigerator room floor drain located at the threshold.

	A.	Floor Drain:
		1.	Model: No. 2586 (-G-NB). 
		2.	Description: Galvanized cast iron drain and secured grate with nickel bronze top.

**** OR ****

Include the following for a packing house floor drain.

	A.	Floor Drain:
		1.	Model: No. 2488.
		2.	Description: Cast iron drain and cast iron flashing collar with heavy duty ductile iron grate and cast iron sediment bucket.

**** OR ****

Include the following for a planting box drain.

	A.	Floor Drain:
		1.	Model: No. 2675.
		2.	Description: Cast iron drain and cast iron flashing clamp with polyethylene dome and stainless steel mesh screen.
**** OR ****

Include the following for a planting box drain with perforated standpipe.

	A.	Floor Drain:
		1.	Model: No. 2680 or 2685.
		2.	Description: Cast iron drain and cast iron flashing clamp with polished bronze dome and perforated bronze standpipe.

**** OR ****

Include the following for a playground area drain.

	A.	Floor Drain:
		1.	Model: No. 2110 (-U).
		2.	Description: Cast iron drain and cast iron flashing collar with modified vandal proof secured medium duty cast iron grate. 

**** OR ****

Include the following for a side outlet playground area drain.

	A.	Floor Drain:
		1.	Model: No. 2115 (-U).
		2.	Description: Cast iron, side outlet, drain and cast iron flashing collar with modified vandal proof secured medium duty cast iron grate.

**** OR ****

Include the following for a promenade deck drain with light pedestrian traffic.

	A.	Floor Drain:
		1.	Model: No. 1410 (-NB-M).
		2.	Description: Cast iron drain and cast iron flashing clamp with seepage openings and heavy duty secured 1/4 inch square hole nickel bronze grate veneered over ductile iron undergrate.

**** OR ****

Include the following for a promenade deck drain with normal pedestrian traffic.

	A.	Floor Drain:
		1.	Model: No. 1412.
		2.	Description: Cast iron drain and flashing clamp with secured 1/4 inch square hole nickel bronze grate veneered over ductile iron undergrate.

**** OR ****

Include the following for a pedestrian ramp area drain.

	A.	Floor Drain:
		1.	Model: No. 2810.
		2.	Description: Cast iron 6 inch wide x 12 inch long heavy duty drain of lengths and figure numbers as shown on plans.

**** OR ****

Include the following for a sanitary floor drain where normal drainage is anticipated.

	A.	Floor Drain:
		1.	Model: No. 3020 (-C).
		2.	Description: Cast iron 8-1/2 inch diameter drain with acid resistant coated interior with nickel bronze secured grate and nickel bronze rim. Aluminum dome bottom strainer. Flashing clamp 
			(-C) in membrane floors.

**** OR ****

Include the following for a square top sanitary floor drain where normal drainage is anticipated.

	A.	Floor Drain:
		1.	Model: No. 3100 (-C).
		2.	Description: Cast iron, 8-1/2 inch diameter, square top drain with acid resistant coated interior with nickel bronze secured grate and nickel bronze rim. Aluminum dome bottom strainer. Flashing clamp (-C) in membrane floors.

**** OR ****

Include the following for a sanitary floor drain where high capacity drainage is required.

	A.	Floor Drain:
		1.	Model: No. 3061 (-C).
		2.	Description: Cast iron 12-1/2 inch diameter drain with acid resistant coated interior with nickel bronze secured grate and nickel bronze rim. Slotted aluminum sediment bucket. Flashing clamp (-C) in membrane floors.

**** OR ****

Include the following for a square top sanitary floor drain where high capacity drainage is required.

	A.	Floor Drain:
		1.	Model: No. 3151 (-C).
		2.	Description: Cast iron, 12-1/2 inch diameter, 8 inch deep, square top drain with acid resistant coated interior with nickel bronze secured grate and nickel bronze rim. Slotted aluminum sediment bucket. Flashing clamp (-C) in membrane floors.

**** OR ****

Include the following for shower drains for single showers.

	A.	Floor Drain:
		1.	Model: No. 2010 (-NB-B).
		2.	Description: Cast iron drain and cast iron flashing collar, cast iron sediment bucket, with 6 inch square adjustable nickel bronze strainer head.

**** OR ****

Include the following for side outlet shower drains for single showers.

	A.	Floor Drain:
		1.	Model: No. 2015 (-NB-B).
		2.	Description: Cast iron, side outlet, drain and cast iron flashing collar, cast iron sediment bucket, with 6 inch square adjustable nickel bronze strainer head and secured square hole nickel bronze grate.

**** OR ****

Include the following for shower gutter drains for multiple showers.

	A.	Floor Drain:
		1.	Model: No. 2010 (-NB-T-U).
		2.	Description: Cast iron drain and cast iron flashing collar with 5 inch x 17 inch adjustable nickel bronze top with secured vandal proof nickel bronze strainer with small square holes.

**** OR ****

Include the following for side outlet shower gutter drains for multiple showers.

	A.	Floor Drain:
		1.	Model: No. 2015 (-NB-T-U).
		2.	Description: Cast iron, side outlet, drain and cast iron flashing collar with 5 inch x 17 inch adjustable nickel bronze top with secured vandal proof nickel bronze strainer with small square holes.

**** OR ****

Include the following for central shower drains for multiple showers.

	A.	Floor Drain:
		1.	Model: No. 2010 (-NB-B-U).
		2.	Description: Cast iron drain and cast iron flashing collar, cast iron sediment bucket, with 6 inch square adjustable nickel bronze top and secured vandal proof nickel bronze strainer.

**** OR ****

Include the following for side outlet central shower drains for multiple showers.

	A.	Floor Drain:
		1.	Model: No. 2015 (-NB-B-U).
		2.	Description: Cast iron, side outlet, drain and cast iron flashing collar, cast iron sediment bucket, with 6 inch square adjustable nickel bronze top and secured vandal proof nickel bronze strainer.

**** OR ****

Include the following for shower drains at the wall for multiple showers.

	A.	Floor Drain:
		1.	Model: No. 2010 (-CP-W-U).
		2.	Description: Cast iron drain and cast iron flashing collar with 6 inch adjustable chrome plated bronze angle top with secured vandal proof angle chrome plated bronze strainer.

**** OR ****

Include the following for side outlet shower drains at the wall for multiple showers.

	A.	Floor Drain:
		1.	Model: No. 2015 (-CP-W-U).
		2.	Description: Cast iron, side outlet, drain and cast iron flashing collar with 6 inch adjustable chrome plated bronze angle top with secured vandal proof angle chrome plated bronze strainer.

**** OR ****

Include the following for shower drains for the locker area aisles under benches.

	A.	Floor Drain:
		1.	Model: No. 2010 (-NB-M-U).  
		2.	Description: Cast iron drain and cast iron flashing collar with 4 inch x 12 inch adjustable nickel bronze top with secured vandal proof nickel bronze strainer with small square holes. 

**** OR ****

Include the following for side outlet shower drains for the locker area aisles under benches.

	A.	Floor Drain:
		1.	Model: No. 2015 (-NB-M-U). 
		2.	Description: Cast iron, side outlet, drain and cast iron flashing collar with 4 inch x 12 inch adjustable nickel bronze top with secured vandal proof nickel bronze strainer with small square holes. 

**** OR ****

Include the following for shower drains for the entrance to the drying area.

	A.	Floor Drain:
		1.	Model: No. 2010 (-NB-T-U).
		2.	Description: Cast iron drain and cast iron flashing collar with 5 inch x 17 inch adjustable nickel bronze top with secured vandal proof nickel bronze strainer with small square holes. 

**** OR ****

Include the following for side outlet shower drains for the entrance to the drying area.

	A.	Floor Drain:
		1.	Model: No. 2015 (-NB-T-U).
		2.	Description: Cast iron, side outlet, drain and cast iron flashing collar with 5 inch x 17 inch adjustable nickel bronze top with secured vandal proof nickel bronze strainer with small square holes. 

**** OR ****

Include the following for slaughter house floor drains.

	A.	Floor Drain:
		1.	Model: No. 2640 (-RB-G).
		2.	Description: Galvanized cast iron dual blood and water drains with galvanized cast iron flashing collar. Cast bronze tractor grate, cast bronze ground joint plug and two bronze rims. 

**** OR ****

Include the following for toilet room floor drains.

	A.	Floor Drain:
		1.	Model: No. 2010 (-NB-A).
		2.	Description: Cast iron drain and cast iron flashing collar with adjustable 5 inch diameter adjustable nickel bronze top.

**** OR ****

Include the following for side outlet toilet room floor drains.

	A.	Floor Drain:
		1.	Model: No. 2015 (-NB-A).
		2.	Description: Cast iron, side outlet, drain and cast iron flashing collar with adjustable 5 inch diameter adjustable nickel bronze top.

**** OR ****

Include the following for vending machine area floor drains.

	A.	Floor Drain:
		1.	Model: No. 2010 (-NB-D-U).
		2.	Description: Cast iron drain with 7 inch diameter adjustable extra heavy nickel bronze top with secured vandal proof nickel bronze strainer.

**** OR ****

Include the following for side outlet vending machine area floor drains.

	A.	Floor Drain:
		1.	Model: No. 2015 (-NB-D-U).
		2.	Description: Cast iron, side outlet, drain with 7 inch diameter adjustable extra heavy nickel bronze top with secured vandal proof nickel bronze strainer.

**** OR ****

Include the following for warehouse floor drains.

	A.	Floor Drain:
		1.	Model: No. 2140.
		2.	Description: Cast iron 12 inch diameter drain with cast iron flashing collar and heavy duty cast iron tractor grate.

**** OR ****

Include the following for side outlet warehouse floor drains.

	A.	Floor Drain:
		1.	Model: No. 2145.
		2.	Description: Cast iron, side outlet, 12 inch diameter drain with cast iron flashing collar and heavy duty cast iron tractor grate.

**** OR ****

Include the following for water heater room floor drains.

	A.	Floor Drain:
		1.	Model: No. 2110 (-S).
		2.	Description: Cast iron 8-1/2 inch square drain and medium duty cast iron grate.

**** OR ****

Include the following for side outlet water heater room floor drains.

	A.	Floor Drain:
		1.	Model: No. 2115 (-S).
		2.	Description: Cast iron, side outlet, 8-1/2 inch square drain and medium duty cast iron grate.

Insert the following under “Accessories.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting http://www.baldwinhardware.comspecific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a trap primer:

	A.	Trap Primer:
		1.	Model: No. 2699.
		2.	Description: Cast bronze trap primer with 1/2 inch connections.

**** OR ****

Include the following to adapt a trap primer for use with a primered drain:

	A.	Trap Primer Adaptor:
		1.	Model: No. 2695 or 2696.
		2.	Description: Cast iron trap primer adaptor with 1/2 inch NPT tapping.

**** OR ****

Include the following for a backwater valve:

	A.	Backwater Valve:
		1.	Model: No. 7012.
		2.	Description: Cast iron body and bolted cover with bronze backwater valve assembly.

PART 3 - EXECUTION

Include the following under “Installation”:

	A.	Install components in accordance with manufacturer's instructions and approved product data submittals.

	B.	Set plumb, level, and rigid.