TRENCH DRAINS

SUGGESTED SPECIFICATIONS

Jay R. Smith Mfg. Co. has developed the following paragraphs to assist the design professional in specifying trench drains. Insert these paragraphs into project specification Section 22 40 00 - Plumbing Fixtures or other similarly titled section.

Notes are included to assist the design professional in editing the specifications to suit project requirements, and are not intended to be included in the final specification. These notes appear in blue text.

For assistance on the selection of the products in this section or for other questions, contact Jay R. Smith Mfg. Co. by calling 334-277-8520, by email at salesengineering@jrsmith.com, or visit our website at www.jrsmith.com.

PART 1 - GENERAL

Insert the following paragraphs under “Submittals”:

	A.	Review Submittals:
		1.	Product Data: Manufacturer’s standard data sheets describing components including materials, dimensions, relationship to adjacent construction, and attachments.

PART 2 - PRODUCTS

Insert the following under “Manufacturers”. Edit to indicate whether or not substitutions will be permitted for the products in this section.

	A.	Contract Documents are based on products by Jay R. Smith Mfg. Co.

	B.	Substitutions: [Under provisions of Division 01.] [Not permitted.]

Insert the following under “Components.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting specific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a 6 inch wide modular stainless steel trench drain system.

	A.	Trench Drain:
		1.	Model: No. 9660.
		2.	Description: 16 gauge type 304 stainless steel trench drain system with pre-sloped modular trench drain body sections with leveling studs and bolting end plates, 4 inch no hub bottom outlet at low end, and secured stainless steel slotted grate.

**** OR ****

Include the following for a 6 inch wide modular stainless steel trench drain system for kitchens or other areas where a trough drain is required and sanitation is of prime concern.

	A.	Trench Drain:
		1.	Model: No. 9660-10N.
		2.	Description: 16 gauge type 304 stainless steel trench drain body with leveling studs, bolting end plates, 4 inch no hub center bottom outlet, secured load class C stainless steel bar grate, and stainless steel dome bottom strainer.

	**** OR ****

Include the following for a 6 inch presloped fiberglass trench system where high flow capacity and velocity are required.

	A.	Trench Drain:
		1.	Model: No. 9810.
		2.	Description: 6 inch wide hydraulic presloped fiberglass trench system.

**** OR ****

Include the following for a 10 inch presloped fiberglass trench system where high flow capacity and velocity are required.

	A.	Trench Drain:
		1.	Model: No. 9812.
		2.	Description: 10 inch wide presloped fiberglass trench system.
			
**** OR ****

Include the following for a 6 inch wide channel slope precast polymer concrete system.

	A.	Trench Drain:
		1.	Model: No. 9814.
		2.	Description: 6 inch wide sloped precast polymer concrete channel.

**** OR ****

Include the following for a 6 inch wide channel slope polymer concrete system requiring an extra heavy duty, fully sloped channel system.
		
	A.	Trench Drain:
		1.	Model: No. 9816.
		2.	Description: 6 inch wide extra heavy duty sloped precast polymer concrete channel with ductile iron frame and grate.

**** OR ****

Include the following for a 6 inch wide channel slope precast polymer concrete system with cast-in metal rails.

	A.	Trench Drain:
		1.	Model: No. 9818.
		2.	Description: 6 inch wide sloped precast polymer concrete channel with QuickLock cover grate and rail.

**** OR ****		

Include the following for a 12 inch wide channel slope precast polymer concrete system requiring a high capacity, extra heavy duty, fully sloped channel system.

	A.	Trench Drain:
		1.	Model: No. 9828.
		2.	Description: 12 inch wide channel brute extra heavy duty polymer concrete channel with ductile iron rails. Secured ductile iron slotted or ADA compliant grates.

**** OR ****	
		
Include the following for surface drainage where installation depth is restricted.

	A.	Trench Drain:
		1.	Model: No. 9832.
		2.	Description: 6 inch wide high strength polyester concrete shallow channel system.

**** OR ****	

Include the following for narrow surface drainage where installation depth is restricted.

	A.	Trench Drain:
		1.	Model: No. 9833.
		2.	Description: 3 inch wide precast polyester interlocking concrete channel with non-sloping radius bottom channel and integral galvanized steel rail edge. 

**** OR ****

Include the following for a brickslot trench drain for use with brick or stone pavers.

	A.	Trench Drain:
		1.	Model: No. 9835.
		2.	Description: Galvanized steel grate with quicklock locking device. 

**** OR ****

Include the following for a trench drain where installation depth is restricted.

	A.	Trench Drain:
		1.	Model: No. 9836.
		2.	Description: 5 inch wide precast polyester interlocking concrete channel with non-sloping flat bottom channel and integral galvanized steel rail edge.

**** OR ****

Include the following for a membrane drain with waterproofing clamping system.

	A.	Trench Drain:
		1.	Model: No. 9837.
		2.	Description: Polyester polymer concrete clamping subframe with integrally molded galvanized steel edge rails and galvanized steel clamping devices.

**** OR ****

Include the following for a 6 inch wide polypropylene trench drain system for light and heavy duty applications.

	A.	Trench Drain:
		1.	Model: No. 9930.
		2.	Description: 6 inch wide presloped drainage system with 100 percent polypropylene interlocking channels with radiused bottom, with Quicklock cover grate.

**** OR ****
	
Include the following for a 6 inch wide polypropylene trench drain system requiring a heavy duty frame, grate and fully sloped channel.
.
	A.	Trench Drain:
		1.	Model: No. 9931.
		2.	Description: 6 inch wide presloped drainage system with 100 percent polypropylene interlocking channels, radiused bottom, and ductile iron frame with concrete frame anchors and ductile iron grate.

Insert the following under “Accessories.” Refer to the Jay R. Smith Mfg. Co. catalog or website for assistance in selecting http://www.jrsmith.com specific model numbers, then select and edit the following paragraphs accordingly.

Include the following for a catch basin for use with a fiberglass trench drain system for load class E.
.
	A.	Catch Basin:
		1.	Model: No. 9812-880-CBM 24, 9812-660-CBM 12.	
		2.	Description: Polyester resin fiberglass catch basin with duco coated steel frame, integral installation brackets, and secured ductile iron slotted grate.
				
**** OR ****		

Include the following for a modular polymer concrete catch basin.
.
	A.	Catch Basin:
		1.	Model: No. 9864-TM.	
		2.	Description: Precast polymer concrete catch basin with ductile iron frame, ductile iron slotted grate, preformed knockout panels, and preformed 6 inch outlet knockouts.
				
**** OR ****

Include the following for a sump box for use with any of the channel slope precast polymer concrete systems.
.
	A.	Sump Box:
		1.	Model: No. 9846.	
		2.	Description: Polymer concrete sump box with cast iron frame and loose set cast iron slotted grate.
				
**** OR ****		

Include the following for a rante-arrow for the 9930 and 9931 drainage systems.
.
	A.	Rante-Arrow:
		1.	Model: No. 9849.	
		2.	Description: Rante-arrow.
			
**** OR ****

Include the following for a channel brace for the 9814 and 9818 drainage systems.
.
	A.	Channel Brace:
		1.	Model: No. 9851.	
		2.	Description: Channel brace.
				
**** OR ****

Include the following for a channel brace for 4 inch inside diameter polymer concrete trench systems.
.
	A.	Channel Chair:
		1.	Model: No. 9852.	
		2.	Description: Channel chair.
				
**** OR ****

Include the following for a shovel head for 4 inch inside diameter channels.
.
	A.	Shovel Head:
		1.	Model: No. 9853.	
		2.	Description: Shovel head.
				
**** OR ****

Include the following for a strainer for 4 inch diameter channel outlet hole.
.
	A.	Strainer:
		1.	Model: No. 9854.	
		2.	Description: Strainer.
**** OR ****

Include the following for an oil separator for use in auto body shops, gas stations, and manufacturing and food processing plants, with a light duty load rating (load class A).
.
	A.	Oil Separator:
		1.	Model: No. 9857.	
		2.	Description: Double-basin 220 gallon capacity polyester polymer concrete with required 4 inch PVC piping and 1/4 inch steel diamond cover plates with carbonic zinc coating.
				
**** OR ****		

Include the following for a catch basin for use with 9814 or 9818 Channel Systems.
.
	A.	Catch Basin:
		1.	Model: No. 9860 or No. 9868.	
		2.	Description: Precast polymer concrete catch basin with preformed 4 inch and 6 inch knockouts.
				
**** OR ****		

Include the following for a modular catch basin for use with 9814 or 9818 Channel Systems.
.
	A.	Catch Basin:
		1.	Model: No. 9864-TM.	
		2.	Description: Modular precast polymer concrete catch basin with ductile iron frame, secured ductile iron slotted grate, preformed knockout panels on each side for connection to channels, and preformed 4 inch, 6 inch and 8 inch outlet knockouts.
								
**** OR ****

Include the following for a double arrow channel support for the 9814, 9816, and 9818 drainage systems.
.
	A.	Channel Support:
		1.	Model: No. 9869-D.	
		2.	Description: Double arrow channel support.
				
**** OR ****	

Include the following for a rebar channel support stand.
.
	A.	Channel Support:
		1.	Model: No. 9869-R.	
		2.	Description: Rebar channel support stand.

**** OR ****

Include the following for a light, heavy or extra heavy duty grate for the 9810, 9814, 9818, 9832, 9930, or 9931 Drainage Systems.
.
	A.	Grate:
		1.	Model: No. 9870 series.	
		2.	Description: [Light] [Heavy] [Extra heavy] duty grate.
															
**** OR ****

Include the following for a stainless steel rail for 9930 trench drains.
.
	A.	Rail:
		1.	Model: No. 9930-SSR.	
		2.	Description: Stainless steel rail.

Include the following for an end frame for 9931 trench drains.
.
	A.	End Frame:
		1.	Model: No. 9931-EF.	
		2.	Description: End frame with ductile iron finish.
						
**** OR ****

Include the following for a catch basin for use with 9930 Channel Systems.
.
	A.	Catch Basin:
		1.	Model: No. 9935.	
		2.	Description: Polypropylene molded catch basin with 4 inch and 6 inch preformed no hub outlet connection and secured grate.
				
**** OR ****	

Include the following for a catch basin for use with 9931 Channel Systems.
.
	A.	Catch Basin:
		1.	Model: No. 9936.	
		2.	Description: Polypropylene molded catch basin with 4 inch and 6 inch preformed no hub outlet connection, ductile iron frame, galvanized concrete anchors, and secured grate.
								
PART 3 - EXECUTION											

Include the following under “Installation”:

	A.	Install components in accordance with manufacturer's instructions and approved product data submittals.

	B.	Set plumb, level, and rigid.